BLE commands

# Steps:

1. Initialize your serial tool at 9600 baudrate
2. Send ble initialize command with or without passkey(BLE\_INIT\_WITH\_PASSKEY\_443322 or BLE\_INIT)
3. You will see the device when you scan after initialization